SdFat: Class Hierarchy

SdFat

Class Hierarchy

Go to the graphical class hierarchy

This inheritance list is sorted roughly, but not completely, alphabetically:
[detail level 12345]

▼C BaseBlockDriver | Base block driver
▼C SdioCard | Raw SDIO access to SD and SDHC flash memory cards
C SdioCardEX | Extended SD I/O block driver
C biosParmBlock | BIOS parameter block
C cache_t | Cache for an raw data block
C directoryEntry | FAT short directory entry
C fat32_boot | Boot sector for a FAT32 volume
C fat32_fsinfo | FSINFO sector for a FAT32 volume
C fat_boot | Boot sector for a FAT12/FAT16 volume
C FatCache | Block cache
▼C FatFile | Basic file class
▼C FatStreamBase | Base class for C++ style streams
C fstream | File input/output stream
C ifstream | File input stream
C ofstream | File output stream
C File | Arduino SD.h style File API
▼C PrintFile | FatFile with Print
C SdFile | Class for backward compatibility
C SdBaseFile | Class for backward compatibility
C StdioStream | StdioStream implements a minimal stdio stream
C FatPos_t | Internal type for file position - do not use in user apps
▼C FatVolume | Access FAT16 and FAT32 volumes on raw file devices
▼C FatFileSystem | Integration class for the FatLib library
C SdFileSystem< SdDriverClass > | Virtual base class for SdFat library
▼C SdFileSystem< SdioCard > |
C SdFatSdio | SdFat class using SDIO
▼C SdFileSystem< SdioCardEX > |
C SdFatSdioEX | SdFat class using SDIO
▼C SdFileSystem< SdSpiCard > |
C SdFat | Main file system class for SdFat library
C SdFatSoftSpi< MisoPin, MosiPin, SckPin > | SdFat class using software SPI
▼C SdFileSystem< SdSpiCardEX > |
C SdFatEX | SdFat class with extended SD I/O
C SdFatSoftSpiEX< MisoPin, MosiPin, SckPin > | SdFat class using software SPI and extended SD I/O
C fname_t | Internal type for Short File Name - do not use in user apps
▼C ios_base | Base class for all streams
▼C ios | Error and state information for all streams
C FatStreamBase | Base class for C++ style streams
▼C istream | Input Stream
▼C ibufstream | Parse a char string
C ArduinoInStream | Input stream for Arduino Stream objects
C ifstream | File input stream
▼C iostream | Input/Output stream
C fstream | File input/output stream
▼C ostream | Output Stream
C ArduinoOutStream | Output stream for Arduino Print objects
C iostream | Input/Output stream
C obufstream | Format a char string
C ofstream | File output stream
C longDirectoryEntry | FAT long directory entry
C masterBootRecord | Master Boot Record
C partitionTable | MBR partition table entry
▼CPrint |
C MinimumSerial | Mini serial class for the SdFat library
C PrintFile | FatFile with Print
▼C SdSpiCard | Raw access to SD and SDHC flash memory cards via SPI protocol
C Sd2Card | Raw access to SD and SDHC card using default SPI library
C SdSpiCardEX | Extended SD I/O block driver
C setfill | Type for setfill manipulator
C setprecision | Type for setprecision manipulator
C setw | Type for setw manipulator
▼CStream |
C File | Arduino SD.h style File API
C SysCall | SysCall - Class to wrap system calls