SdFat: Class List

SdFat

Class List
Here are the classes, structs, unions and interfaces with brief descriptions:

C ArduinoInStream | Input stream for Arduino Stream objects
C ArduinoOutStream | Output stream for Arduino Print objects
C BaseBlockDriver | Base block driver
C biosParmBlock | BIOS parameter block
C cache_t | Cache for an raw data block
C directoryEntry | FAT short directory entry
C fat32_boot | Boot sector for a FAT32 volume
C fat32_fsinfo | FSINFO sector for a FAT32 volume
C fat_boot | Boot sector for a FAT12/FAT16 volume
C FatCache | Block cache
C FatFile | Basic file class
C FatFileSystem | Integration class for the FatLib library
C FatPos_t | Internal type for file position - do not use in user apps
C FatStreamBase | Base class for C++ style streams
C FatVolume | Access FAT16 and FAT32 volumes on raw file devices
C File | Arduino SD.h style File API
C fname_t | Internal type for Short File Name - do not use in user apps
C fstream | File input/output stream
C ibufstream | Parse a char string
C ifstream | File input stream
C ios | Error and state information for all streams
C ios_base | Base class for all streams
C iostream | Input/Output stream
C istream | Input Stream
C longDirectoryEntry | FAT long directory entry
C masterBootRecord | Master Boot Record
C MinimumSerial | Mini serial class for the SdFat library
C obufstream | Format a char string
C ofstream | File output stream
C ostream | Output Stream
C partitionTable | MBR partition table entry
C PrintFile | FatFile with Print
C Sd2Card | Raw access to SD and SDHC card using default SPI library
C SdBaseFile | Class for backward compatibility
C SdFat | Main file system class for SdFat library
C SdFatEX | SdFat class with extended SD I/O
C SdFatSdio | SdFat class using SDIO
C SdFatSdioEX | SdFat class using SDIO
C SdFatSoftSpi | SdFat class using software SPI
C SdFatSoftSpiEX | SdFat class using software SPI and extended SD I/O
C SdFile | Class for backward compatibility
C SdFileSystem | Virtual base class for SdFat library
C SdioCard | Raw SDIO access to SD and SDHC flash memory cards
C SdioCardEX | Extended SD I/O block driver
C SdSpiCard | Raw access to SD and SDHC flash memory cards via SPI protocol
C SdSpiCardEX | Extended SD I/O block driver
C setfill | Type for setfill manipulator
C setprecision | Type for setprecision manipulator
C setw | Type for setw manipulator
C StdioStream | StdioStream implements a minimal stdio stream
C SysCall | SysCall - Class to wrap system calls